IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "model.ifc"
Time stamp: "2023-08-22T11:39:13+01:00"
Preprocessor: "IfcOpenShell v0.7.0-fc50bdd3a"
Originating system: "BlenderBIM 0.0.230816"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "62 Brown Street"
      contains 1 element
        1 x IFCANNOTATION | names: "2d survey"
      IFCBUILDINGSTOREY "Ground Floor"
        contains 14 elements
          9 x IFCWALL | type IFCWALLTYPE "Exrernal wall metric" | names: "Wall" | material: layers ("Brick metric" 0.224999994039536) | property sets: EPset_Parametric
          1 x IFCDOOR | type IFCDOORTYPE "Doube asym" | names: "Door"
          1 x IFCDOOR | type IFCDOORTYPE "Single external" | names: "Door"
          2 x IFCWALL | type IFCWALLTYPE "Internal stud wall" | names: "Wall" | material: layers "stud wall" ("Stud" 0.100000001490116) | property sets: EPset_Parametric
          1 x IFCDOOR | type IFCDOORTYPE "Single internal" | names: "Door"

Types
  IFCWALLTYPE "Exrernal wall metric" | STANDARD | 9 occurrences | material: layers ("Brick metric" 0.224999994039536)
  IFCDOORTYPE "Doube asym" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | property sets: BBIM_Door
  IFCDOORTYPE "Single external" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door
  IFCWALLTYPE "Internal stud wall" | STANDARD | 2 occurrences | material: layers "stud wall" ("Stud" 0.100000001490116) | property sets: Pset_WallCommon
  IFCDOORTYPE "Single internal" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door, Pset_DoorCommon

Property sets
  EPset_Parametric | properties | on 11 objects (11 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "DOUBLE_DOOR_SINGLE_SWING", "overall_height": 2.0, "overall_width": 1.399999976158142, "lining_properties": {"lining_depth": 0.14000000059604645, "lining_thickness": 0.05000000074505806, "lining_offset": 0.08500000089406967, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 0.8999999761581421, "lining_properties": {"lining_depth": 0.14000000059604645, "lining_thickness": 0.05000000074505806, "lining_offset": 0.08500000089406967, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 0.7599999904632568, "lining_properties": {"lining_depth": 0.10000000149011612, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  Pset_WallCommon | properties | on 1 type object
    Compartmentation = FALSE (IFCBOOLEAN)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_DoorCommon | properties | on 1 type object
    Status in {"EXISTING"} (IFCLABEL)