IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "model.ifc"
Time stamp: "2025-01-22T11:41:01+00:00"
Preprocessor: "IfcOpenShell 0.8.1-alpha250121"
Originating system: "Bonsai 0.8.1-alpha250121-c72f170"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site" | latitude 53° 23′ 0″ | longitude 1° 28′ 0″ | elevation above sea level 75.
    IFCBUILDING "62 Brown Street"
      contains 1 element
        1 x IFCANNOTATION | names: "2d survey"
      IFCBUILDINGSTOREY "Ground Floor"
        contains 55 elements
          2 x IFCWALL | type IFCWALLTYPE "Internal stud wall" | names: "Wall" | material: layers "stud wall" ("Stud" 0.100000001490116) | property sets: EPset_Parametric
          6 x IFCSLAB | type IFCSLABTYPE "concrete slab" | names: "Slab" | material: layers "solid slab 250" ("Concrete" 0.25) | property sets: EPset_Parametric
          13 x IFCWALL | type IFCWALLTYPE "External wall metric" | names: "Wall" | material: layers "solid brick 225" ("Brick" 0.224999994039536) | property sets: EPset_Parametric, BBIM_Boolean, Qto_WallBaseQuantities
          2 x IFCDOOR | type IFCDOORTYPE "Single internal" | names: "Door"
          6 x IFCSTAIRFLIGHT | type IFCSTAIRFLIGHTTYPE "steps" | STRAIGHT | names: "StairFlight" | material: "Concrete" | property sets: Pset_StairFlightCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "280 wide" | TRIPLE_PANEL_VERTICAL | names: "Window"
          3 x IFCWINDOW | type IFCWINDOWTYPE "104 wide" | names: "Window"
          1 x IFCDOOR | type IFCDOORTYPE "external short" | SINGLE_SWING_LEFT | names: "Door"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "30 square" | names: "Column" | material: profiles ("Concrete") | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "800 wide" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          2 x IFCWALL | type IFCWALLTYPE "External wall Victorian" | names: "Wall" | material: layers "brick 350" ("Brick" 0.349999994039536) | property sets: EPset_Parametric
          1 x IFCBEAM | type IFCBEAMTYPE "30 square" | names: "Beam" | material: profiles ("Concrete") | property sets: EPset_Parametric
          1 x IFCDOOR | type IFCDOORTYPE "104 wide" | SINGLE_SWING_LEFT | names: "Door"
          3 x IFCCOVERING | type IFCCOVERINGTYPE "Facade trim" | names: "Covering" | material: profiles "cowl" ("Concrete") | property sets: EPset_Parametric
          2 x IFCSLAB | type IFCSLABTYPE "Crinkly roof" | names: "Slab" | material: layers ("Concrete" 0.100000001490116) | property sets: EPset_Parametric
          2 x IFCWALL | type IFCWALLTYPE "Internall wall Victorian" | names: "Wall" | material: layers ("Brick" 0.1) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "130 wide" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          1 x IFCDOOR | type IFCDOORTYPE "Doube asym" | DOUBLE_DOOR_SINGLE_SWING | names: "Door"
          1 x IFCWINDOW | type IFCWINDOWTYPE "110 wide" | DOUBLE_PANEL_VERTICAL | names: "Window"
          3 x IFCWINDOW | type IFCWINDOWTYPE "104 wide" | TRIPLE_PANEL_HORIZONTAL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "70 wide" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          1 x IFCDOOR | type IFCDOORTYPE "Single external" | names: "Door"
        IFCSPACE "Centre downstairs" | INTERNAL
          contains 4 elements
            4 x IFCCOLUMN | type IFCCOLUMNTYPE "30 square" | names: "Column" | material: profiles ("Concrete") | property sets: EPset_Parametric
      IFCBUILDINGSTOREY "First floor"
        contains 71 elements
          2 x IFCWINDOW | type IFCWINDOWTYPE "130 wide" | names: "Window"
          26 x IFCWALL | type IFCWALLTYPE "External wall metric" | names: "Wall" | material: layers "solid brick 225" ("Brick" 0.224999994039536) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "55 wide full height" | names: "Window"
          2 x IFCDOOR | type IFCDOORTYPE "External 160 double" | DOUBLE_DOOR_SINGLE_SWING | names: "Door"
          6 x IFCSLAB | type IFCSLABTYPE "concrete slab" | names: "Slab" | material: layers "solid slab 250" ("Concrete" 0.25) | property sets: EPset_Parametric, EPset_Drawing
          1 x IFCWALL | type IFCWALLTYPE "Tiled external wall" | names: "Wall" | material: layers "tiled wall" ("Tile cladding" 0.0199999995529652) | property sets: EPset_Parametric
          4 x IFCWINDOW | type IFCWINDOWTYPE "61 wide" | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "180 wide" | DOUBLE_PANEL_VERTICAL | names: "Window"
          2 x IFCWALL | type IFCWALLTYPE "External wall Victorian" | names: "Wall" | material: layers "brick 350" ("Brick" 0.349999994039536) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "800 wide" | names: "Window"
          2 x IFCWINDOW | type IFCWINDOWTYPE "104 wide short" | DOUBLE_PANEL_HORIZONTAL | names: "Window"
          3 x IFCDOOR | type IFCDOORTYPE "Single internal" | names: "Door"
          1 x IFCWINDOW | type IFCWINDOWTYPE "61 wide" | SINGLE_PANEL | names: "Window"
          1 x IFCWINDOW | type IFCWINDOWTYPE "55 wide full height" | SINGLE_PANEL | names: "Window"
          7 x IFCWINDOW | type IFCWINDOWTYPE "104 wide short" | names: "Window"
          3 x IFCWALL | type IFCWALLTYPE "Internal stud wall" | names: "Wall" | material: layers "stud wall" ("Stud" 0.100000001490116) | property sets: EPset_Parametric
          1 x IFCWINDOW | type IFCWINDOWTYPE "280 wide" | TRIPLE_PANEL_VERTICAL | names: "Window"
          3 x IFCBEAM | type IFCBEAMTYPE "Shed truss" | names: "Beam"
          1 x IFCSTAIRFLIGHT | type IFCSTAIRFLIGHTTYPE "steps" | STRAIGHT | names: "StairFlight" | material: "Concrete" | property sets: Pset_StairFlightCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Coping cornice" | names: "Covering" | material: profiles "cornice" ("Concrete") | property sets: EPset_Parametric
          2 x IFCWALL | type IFCWALLTYPE "Internall wall Victorian" | names: "Wall" | material: layers ("Brick" 0.1) | property sets: EPset_Parametric
        IFCSPACE "Centre upstairs" | INTERNAL
          contains 5 elements
            2 x IFCCOLUMN | type IFCCOLUMNTYPE "30 square" | names: "Column" | material: profiles ("Concrete") | property sets: EPset_Parametric
            2 x IFCBEAM | type IFCBEAMTYPE "30 square" | names: "Beam" | material: profiles ("Concrete") | property sets: EPset_Parametric
            1 x IFCWALL | type IFCWALLTYPE "Internall wall Victorian" | names: "Wall" | material: layers ("Brick" 0.1) | property sets: EPset_Parametric

Types
  IFCWALLTYPE "Internal stud wall" | STANDARD | 5 occurrences | material: layers "stud wall" ("Stud" 0.100000001490116) | property sets: Pset_WallCommon
  IFCSLABTYPE "concrete slab" | FLOOR | 12 occurrences | material: layers "solid slab 250" ("Concrete" 0.25) | property sets: EPset_Parametric
  IFCWALLTYPE "External wall metric" | STANDARD | 39 occurrences | material: layers "solid brick 225" ("Brick" 0.224999994039536)
  IFCDOORTYPE "Single internal" | DOOR | SINGLE_SWING_LEFT | 5 occurrences | property sets: BBIM_Door, Pset_DoorCommon
  IFCSTAIRFLIGHTTYPE "steps" | STRAIGHT | 7 occurrences | property sets: BBIM_Stair
  IFCWINDOWTYPE "280 wide" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "104 wide" | WINDOW | SINGLE_PANEL | 6 occurrences | property sets: BBIM_Window
  IFCDOORTYPE "external short" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door
  IFCCOLUMNTYPE "30 square" | COLUMN | 7 occurrences | material: profiles ("Concrete")
  IFCWINDOWTYPE "800 wide" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 2 occurrences | property sets: BBIM_Window
  IFCWALLTYPE "External wall Victorian" | SOLIDWALL | 4 occurrences | material: layers "brick 350" ("Brick" 0.349999994039536)
  IFCBEAMTYPE "30 square" | BEAM | 3 occurrences | material: profiles ("Concrete")
  IFCDOORTYPE "104 wide" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door
  IFCCOVERINGTYPE "Facade trim" | CLADDING | 3 occurrences | material: profiles "cowl" ("Concrete")
  IFCSLABTYPE "Crinkly roof" | ROOF | 2 occurrences | material: layers ("Concrete" 0.100000001490116) | property sets: EPset_Parametric
  IFCWALLTYPE "Internall wall Victorian" | SOLIDWALL | 5 occurrences | material: layers ("Brick" 0.1)
  IFCWINDOWTYPE "130 wide" | WINDOW | SINGLE_PANEL | 3 occurrences | property sets: BBIM_Window
  IFCDOORTYPE "Doube asym" | DOOR | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | property sets: BBIM_Door
  IFCWINDOWTYPE "110 wide" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCWINDOWTYPE "70 wide" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCDOORTYPE "Single external" | DOOR | SINGLE_SWING_LEFT | 1 occurrence | property sets: BBIM_Door
  IFCWINDOWTYPE "55 wide full height" | WINDOW | SINGLE_PANEL | 2 occurrences | property sets: BBIM_Window
  IFCDOORTYPE "External 160 double" | DOOR | SINGLE_SWING_LEFT | 2 occurrences | property sets: BBIM_Door
  IFCWALLTYPE "Tiled external wall" | STANDARD | 1 occurrence | material: layers "tiled wall" ("Tile cladding" 0.0199999995529652)
  IFCWINDOWTYPE "61 wide" | WINDOW | SINGLE_PANEL | 5 occurrences | property sets: BBIM_Window
  IFCWINDOWTYPE "180 wide" | WINDOW | SINGLE_PANEL | 1 occurrence | property sets: BBIM_Window
  IFCWINDOWTYPE "104 wide short" | element type "ELEMENTEDWALL" | USERDEFINED | SINGLE_PANEL | 9 occurrences | property sets: BBIM_Window
  IFCBEAMTYPE "Shed truss" | element type "TRUSS" | USERDEFINED | 3 occurrences
  IFCCOVERINGTYPE "Coping cornice" | ROOFING | 1 occurrence | material: profiles "cornice" ("Concrete")

Property sets
  EPset_Parametric | properties | on 52 objects (52 IFCWALL)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 14 objects (7 IFCCOLUMN, 4 IFCCOVERING, 3 IFCBEAM)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 12 objects (12 IFCSLAB)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 objects (2 IFCWALL)
    Engine = "Bonsai.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 2 objects (2 IFCSLAB)
    Engine = "Bonsai.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 2 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:100" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/100" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCSLAB)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1:100" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/100" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NumberOfRiser = 8. (IFCCOUNTMEASURE)
    NumberOfTreads = 7. (IFCCOUNTMEASURE)
    RiserHeight = 0.1875 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 6. (IFCCOUNTMEASURE)
    NumberOfTreads = 5. (IFCCOUNTMEASURE)
    RiserHeight = 0.166666666666667 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NumberOfRiser = 12. (IFCCOUNTMEASURE)
    NumberOfTreads = 11. (IFCCOUNTMEASURE)
    RiserHeight = 0.180000007152557 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 6. (IFCCOUNTMEASURE)
    NumberOfTreads = 5. (IFCCOUNTMEASURE)
    RiserHeight = 0.180000007152557 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 3. (IFCCOUNTMEASURE)
    RiserHeight = 0.180000007152557 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NumberOfRiser = 7. (IFCCOUNTMEASURE)
    NumberOfTreads = 6. (IFCCOUNTMEASURE)
    RiserHeight = 0.179999998637608 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  BBIM_Boolean | properties | on 1 object (1 IFCWALL)
    Data = "[31973]" (IFCTEXT)
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossSideArea = 1.11000391945822 [SQUARE_METRE]
    GrossVolume = 0.215039359747037 [CUBIC_METRE]
    Height = 0.75 [METRE]
    Length = 1.94930650899559 [METRE]
    NetSideArea = 1.11000391945822 [SQUARE_METRE]
    NetVolume = 0.215039359747037 [CUBIC_METRE]
    Width = 0.224999994039536 [METRE]
  Pset_WallCommon | properties | on 1 type object
    Compartmentation = FALSE (IFCBOOLEAN)
    Status in {"EXISTING"} (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 0.7599999904632568, "lining_properties": {"lining_depth": 0.10000000149011612, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 1.7999999523162842, "overall_width": 0.7599999904632568, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.07500000298023224, "casing_depth": 0.004999999888241291, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.75, "overall_width": 1.0449999570846558, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.02500000037252903, "lining_offset": 0.15000000596046448, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "DOUBLE_DOOR_SINGLE_SWING", "overall_height": 2.700000047683716, "overall_width": 1.399999976158142, "lining_properties": {"lining_depth": 0.14000000059604645, "lining_thickness": 0.05000000074505806, "lining_offset": 0.08500000089406967, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "SINGLE_SWING_LEFT", "overall_height": 2.0, "overall_width": 0.8999999761581421, "lining_properties": {"lining_depth": 0.14000000059604645, "lining_thickness": 0.05000000074505806, "lining_offset": 0.08500000089406967, "lining_to_panel_offset_x": 0.05000000074505806, "lining_to_panel_offset_y": 0.0, "transom_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  BBIM_Door | properties | on 1 type object
    Data = "{"door_type": "DOUBLE_DOOR_SINGLE_SWING", "overall_height": 2.0, "overall_width": 1.600000023841858, "lining_properties": {"lining_depth": 0.10000000149011612, "lining_thickness": 0.05000000074505806, "lining_offset": 0.0, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.0, "casing_thickness": 0.0, "threshold_thickness": 0.02500000037252903, "threshold_depth": 0.10000000149011612, "threshold_offset": 0.0}, "panel_properties": {"panel_depth": 0.03500000014901161, "panel_width_ratio": 1.0}}" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 type object
    Status in {"EXISTING"} (IFCLABEL)
  BBIM_Stair | properties | on 1 type object
    Data = "{"stair_type": "CONCRETE", "width": 1.100000023841858, "height": 1.0, "number_of_treads": 5, "tread_run": 0.25, "nosing_length": 0.0, "nosing_depth": 0.0, "base_slab_depth": 0.0, "top_slab_depth": 0.25, "has_top_nib": true, "tread_depth": 0.25, "custom_first_last_tread_run": [0.0, 0.0]}" (IFCTEXT)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_VERTICAL", "overall_height": 1.125, "overall_width": 2.799999952316284, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.02500000037252903, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.019999999552965164, "first_mullion_offset": 0.8999999761581421, "second_mullion_offset": 1.7999999523162842}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "TRIPLE_PANEL_HORIZONTAL", "overall_height": 2.75, "overall_width": 1.0449999570846558, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.02500000037252903, "lining_offset": 0.15000000596046448, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.699999988079071, "second_transom_offset": 1.0}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 1.2999999523162842, "overall_width": 0.800000011920929, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.800000011920929}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 1.2999999523162842, "overall_width": 1.2999999523162842, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.800000011920929}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_VERTICAL", "overall_height": 1.7000000476837158, "overall_width": 1.100000023841858, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "mullion_thickness": 0.019999999552965164, "first_mullion_offset": 0.550000011920929}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "DOUBLE_PANEL_HORIZONTAL", "overall_height": 1.0499999523162842, "overall_width": 0.699999988079071, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903, "transom_thickness": 0.05000000074505806, "first_transom_offset": 0.6000000238418579}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 2.0, "overall_width": 0.550000011920929, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window | properties | on 1 type object
    Data = "{"window_type": "SINGLE_PANEL", "overall_height": 0.824999988079071, "overall_width": 0.6100000143051147, "lining_properties": {"lining_depth": 0.05000000074505806, "lining_thickness": 0.05000000074505806, "lining_offset": 0.05000000074505806, "lining_to_panel_offset_x": 0.02500000037252903, "lining_to_panel_offset_y": 0.02500000037252903}, "panel_properties": {"frame_depth": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161], "frame_thickness": [0.03500000014901161, 0.03500000014901161, 0.03500000014901161]}}" (IFCLABEL)
  BBIM_Window: 2 more contents on 0 objects not shown